|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Bridge Name: Harper Avenue** | | **Bridge type: Single span** | | **Highway/Road Carlton Mill / Rolleston Ave** | **RP:** | **BSN: CC23** |
| Deck width: 10 m | | | GPS (lat,long): -43.5208303,172.6255355 | | | |
| Total Bridge length: 16 m | | | Owner: Christchurch City Council | | | |
| Span: 1 of 1 | | | Weather: Sunny, Fine | | | |
| Span length: 16 m | | |  | | | |
| Inspector: Mark English | | | Inspection type: Routine | | | |
| Date: 01-Jun-2016 | Date (mth/yr): | | Next inspection type: General | | | |

|  |  |
| --- | --- |
| **Photos** | |
| **Item no.** | **Element, remedial work and element photos** |
| 1. **1** | Secondary - Other (incl. deck) - Scheduled maintenance (Medium)  Resurface and investigate drop   |  |  |  | | --- | --- | --- | |  |  |  | |
| 1. **1** | Abutments - Routine maintenance (High)  Investigate cracks  Reskim concrete   |  |  |  | | --- | --- | --- | |  |  |  | |
| 1. **1** | Painting : Barriers / guardrails - Scheduled maintenance (Low)  Scrub and clean   |  |  |  | | --- | --- | --- | |  |  |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. **1** | Access / walkways / gantries - Scheduled maintenance (Medium)  Chipp off spilled concrete   |  |  |  | | --- | --- | --- | |  |  |  | |
| 1. **1** | Guardrail / handrail / safety fences - Scheduled maintenance (High)  Fix guard fence in place.   |  |  |  | | --- | --- | --- | |  |  |  | |

|  |
| --- |
| **Supporting Photos** |



Bealey Ave approach



Riverbed upstream



Side view of span



Erosion protection