|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Bridge Name:Harper Avenue** | **Bridge type:Single span** | **Highway/RoadCarlton Mill / Rolleston Ave** | **RP:** | **BSN:CC23** |
| Deck width: 10 m | GPS (lat,long): -43.5208303,172.6255355 |
| Total Bridge length: 16 m | Owner: Christchurch City Council |
| Span: 1 of 1 | Weather: Sunny, Fine |
| Span length: 16 m |  |
| Inspector: Mark English | Inspection type: Routine |
| Date: 01-Jun-2016 | Date (mth/yr):  | Next inspection type: General |

|  |
| --- |
| **Photos** |
| **Item no.** | **Element, remedial work and element photos** |
| 1. **1**
 | Secondary - Other (incl. deck) - Scheduled maintenance (Medium)Resurface and investigate drop

|  |  |  |
| --- | --- | --- |
|  |  |  |

 |
| 1. **1**
 | Abutments - Routine maintenance (High)Investigate cracksReskim concrete

|  |  |  |
| --- | --- | --- |
|  |  |  |

 |
| 1. **1**
 | Painting : Barriers / guardrails - Scheduled maintenance (Low)Scrub and clean

|  |  |  |
| --- | --- | --- |
|  |  |  |

 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1. **1**
 | Access / walkways / gantries - Scheduled maintenance (Medium)Chipp off spilled concrete

|  |  |  |
| --- | --- | --- |
|  |  |  |

 |
| 1. **1**
 | Guardrail / handrail / safety fences - Scheduled maintenance (High)Fix guard fence in place.

|  |  |  |
| --- | --- | --- |
|  |  |  |

 |

|  |
| --- |
| **Supporting Photos** |



Bealey Ave approach



Riverbed upstream



Side view of span



Erosion protection