|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Wall name: Memorial wall** | | **Wall type: Precast concrete** | | **Highway/Road Kilmore and Manchester** | **RP: 15263** | **OSN: FG 234** |
| Length: 50 m | | | GPS (lat,long): -43.5266818,172.6422713 | | | |
| Max height: 0.75 m | | | Owner: Local Authority | | | |
| Average height: 0.75 | | | Weather: Sunny, Fine | | | |
| Angle to vertical: 0 ˚ | | | Offset from highway centreline: 6.5 m | | | |
| Retained material: Earthworks, second wall for path. | | | | | | |
| Inspector: Mark English | | | Inspection type: Routine | | | |
| Date: 22-Jul-2016 | Date (mth/yr): | | Next inspection type: General | | | |

|  |  |
| --- | --- |
| **Photos** | |
| **Item no.** | **Element, remedial work and element photos** |
| 1. **1** | Retaining wall - Primary - Routine maintenance (Low)  Regular spray with moss killer   |  |  |  | | --- | --- | --- | |  |  |  | |
| 1. **1** | Carriageway - Top of wall - Scheduled maintenance (Medium)  Re-fit anti-skateboard cleats.   |  |  |  | | --- | --- | --- | |  |  |  | |

|  |
| --- |
| **Supporting Photos** |



Guardrail



General view of structure.