|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Wall name:Memorial wall** | **Wall type:Precast concrete** | **Highway/RoadKilmore and Manchester** | **RP:15263** | **OSN:FG 234** |
| Length: 50 m | GPS (lat,long): -43.5266818,172.6422713 |
| Max height: 0.75 m | Owner: Local Authority |
| Average height: 0.75 | Weather: Sunny, Fine |
| Angle to vertical: 0 ˚ | Offset from highway centreline: 6.5 m |
| Retained material: Earthworks, second wall for path. |
| Inspector: Mark English | Inspection type: Routine |
| Date: 22-Jul-2016 | Date (mth/yr):  | Next inspection type: General |

|  |
| --- |
| **Photos** |
| **Item no.** | **Element, remedial work and element photos** |
| 1. **1**
 | Retaining wall - Primary - Routine maintenance (Low)Regular spray with moss killer

|  |  |  |
| --- | --- | --- |
|  |  |  |

 |
| 1. **1**
 | Carriageway - Top of wall - Scheduled maintenance (Medium)Re-fit anti-skateboard cleats.

|  |  |  |
| --- | --- | --- |
|  |  |  |

 |

|  |
| --- |
| **Supporting Photos** |



Guardrail



General view of structure.